{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["(3)新锐志正版PDS检查表","(1)通用正版PDS检查表","（2）新皇冠用PDS正版检查表"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"(3)新锐志正版PDS检查表","index":0,"n_rows":60,"n_cols":18,"rows_kept":60,"cut":false,"hidden":false,"merged":[[0,0,1,17],[51,0,52,1],[53,0,54,1]],"flags":["formulas_cached_only"]}
["锐志新车检查表(PDS)"]
[]
[]
[{"$nulls":8},"调整",{"$nulls":8},"调整"]
["A. 作业准备",{"$nulls":6},"OK","修理","D. 下部检查",{"$nulls":6},"OK","修理"]
["01.轮胎气压计、扭力扳手、21寸套筒、万用表、工具",{"$nulls":8},"01.确认轮胎螺母的扭矩"]
["02.座套、翼子板布、把套、脚垫、布、垫板",{"$nulls":8},"02.调整轮胎的气压"]
["03.安装随车附件",{"$nulls":8},"03.检查轮胎的损坏情况"]
[{"$nulls":9},"04.安装随车附件"]
["B. 目视检查",{"$nulls":8},"05.拆除前弹簧隔垫、制动器防锈罩"]
["01.检查警告灯、蜂鸣器(钥匙、大灯)",{"$nulls":8},"06.检查油液类的渗漏情况"]
["02.检查发动机的起动性、稳定性、异音及振动",{"$nulls":8},"07.检查安装紧固情况"]
["03.电器件的工作状况",{"$nulls":8},"08.检查损伤、生锈情况"]
["    ·  大灯、小灯、雾灯、控制台灯光"]
["    ·  尾灯、牌照灯、后雾灯"]
["    ·  刹车灯、倒车灯、光束调整系统",{"$nulls":8},"E. 路  试"]
["  · 转向灯、双闪",{"$nulls":8},"01.检查踏板的游隙、高度和踩后余量"]
["  · 雨刷器、雨刷喷嘴、喇叭",{"$nulls":8},"02.检查发动机的起动性、平稳性、异响和振动(暖机)"]
["  · 除雾器、点烟器",{"$nulls":8},"03.行驶性能(加速、匀速、减速、灵敏性等)"]
["  · 音响(调频)、时钟(设为正确时间)",{"$nulls":8},"04.检查仪表、指示灯的工作情况"]
["  ·  遮阳板、化妆灯、地图灯",{"$nulls":8},"05.检查传动桥"]
["  ·  室内灯",{"$nulls":8},"06.检查制动性能、异响、驻车制动"]
["    ·  天窗动作",{"$nulls":8},"07.检查转向情况"]
["    ·  座椅加热情况",{"$nulls":8},"08.检查异响、噪音、振动、平稳性"]
["04.检查车内后视镜、门后视镜(调整为正常状态)",{"$nulls":8},"09.检查暖气、空调"]
["05.检查角度及高度可调方向盘动作",{"$nulls":8},"10.自动传动桥的检查"]
["06.检查储物箱及杯架、烟灰缸",{"$nulls":8},"11.检查卫星导航系统"]
["07.检查座椅、安全带的运作、污损情况",{"$nulls":8},"12.检查定速装置工作情况"]
["08.检查发动机盖、后备箱、加油孔盖的开启情况",{"$nulls":8},"13.检查侧方位停车摄像头"]
["09.检查车门玻璃的运作情况"]
["10.检查车门、门锁、遥控门锁、智能系统的工作情况",{"$nulls":8},"F. 最终检查、清洁"]
["11.检查儿童锁",{"$nulls":8},"01.取下不要的标签及覆盖物"]
["12.检查行李箱灯",{"$nulls":8},"02.检查内装部分的安装、污损情况"]
["13.行李箱内衬、垫板的检查",{"$nulls":8},"03.确认驾驶员手册等相关资料（欠品、误品等）"]
["14.检查备胎的气压和安装状况",{"$nulls":8},"04.安装轮毂盖"]
["15.检查千斤顶、工具、三角牌和牵引挂钩等",{"$nulls":8},"05.洗车、驾驶室内清扫"]
["16.引擎盖、车门的安装间隙、段差检查",{"$nulls":8},"06.检查漆面的不良、损坏情况"]
["17.检查驾驶席脚垫(如有)是否正确安装固定",{"$nulls":8},"07.检查外装部分的安装、损坏情况"]
[]
["C. 检查发动机仓"]
["01.检查油液类的量及其质量",{"$nulls":8},"外观备注"]
["  ·   发动机油"]
["  ·  自动传动桥油"]
["  · 制动液"]
["  ·  雨刷清洗液、防冻液"]
["  ·  电瓶液"]
["02.检查油类的渗漏情况"]
["03.检查电瓶桩头的安装情况"]
["04.测量电瓶的电压(                V、标准值12.2)"]
["05.检查电瓶充电情况"]
[]
["工 单 号：",{"$nulls":6},"备注"]
[]
["行驶公里："]
[{"$nulls":5},"KM"]
[]
[]
["检查员:",{"$nulls":6},"质检员:",{"$nulls":5},"服务部长确认:"]
[]
["VIN:",{"$nulls":6},"检查日期:",null,null,null,"经销商名称:",null,"驻马店威龙丰田汽车销售服务有限公司"]

{"sheet":"(1)通用正版PDS检查表","index":1,"n_rows":61,"n_cols":18,"rows_kept":61,"cut":false,"hidden":false,"merged":[[0,0,1,17],[52,0,53,1],[54,0,55,1]],"flags":["formulas_cached_only"]}
["新车检查表(PDS)"]
[]
[]
[{"$nulls":8},"调整",{"$nulls":8},"调整"]
["A. 作业准备",{"$nulls":6},"OK","修理","D. 下部检查",{"$nulls":6},"OK","修理"]
["01.轮胎气压计、扭力扳手、21寸套筒、万用表、工具",{"$nulls":8},"01.确认轮胎螺母的扭矩"]
["02.座套、翼子板布、把套、脚垫、布、垫板",{"$nulls":8},"02.调整轮胎的气压"]
["03.安装随车附件",{"$nulls":8},"03.检查轮胎的损坏情况"]
[{"$nulls":9},"04.安装随车附件"]
["B. 目视检查",{"$nulls":8},"05.拆除前弹簧隔垫、制动器防锈罩"]
["01.检查警告灯、蜂鸣器(钥匙、大灯)",{"$nulls":8},"06.检查油液类的渗漏情况"]
["02.检查发动机的起动性、稳定性、异音及振动",{"$nulls":8},"07.检查安装紧固情况"]
["03.电器件的工作状况",{"$nulls":8},"08.检查损伤、生锈情况"]
["    ·  大灯、小灯、雾灯、控制台灯光"]
["    ·  尾灯、牌照灯、后雾灯"]
["    ·  刹车灯、倒车灯、光束调整系统",{"$nulls":8},"E. 路  试"]
["  · 转向灯、双闪",{"$nulls":8},"01.检查踏板的游隙、高度和踩后余量"]
["  · 雨刷器、雨刷喷嘴、喇叭",{"$nulls":8},"02.检查发动机的起动性、平稳性、异响和振动(暖机)"]
["  · 除雾器、点烟器",{"$nulls":8},"03.行驶性能(加速、匀速、减速、灵敏性等)"]
["  · 音响(调频)、时钟(设为正确时间)",{"$nulls":8},"04.检查仪表、指示灯的工作情况"]
["  ·  遮阳板、化妆灯、地图灯",{"$nulls":8},"05.检查离合器、传动桥"]
["  ·  室内灯",{"$nulls":8},"06.检查制动性能、异响、驻车制动"]
["    ·  天窗动作",{"$nulls":8},"07.检查转向情况"]
["    ·  座椅加热情况",{"$nulls":8},"08.检查异响、噪音、振动、平稳性"]
["04.检查车内后视镜、门后视镜(调整为正常状态)",{"$nulls":8},"09.检查暖气、空调"]
["05.检查角度及高度可调方向盘动作",{"$nulls":8},"10.自动传动桥的检查"]
["06.检查储物箱及杯架、烟灰缸",{"$nulls":8},"11.检查卫星导航系统"]
["07.检查座椅、安全带的运作、污损情况",{"$nulls":8},"12.检查定速装置工作情况"]
["08.检查发动机盖、后备箱、加油孔盖的开启情况"]
["09.检查车门玻璃的运作情况"]
["10.检查车门、门锁、遥控门锁、智能系统的工作情况",{"$nulls":8},"F. 最终检查、清洁"]
["11.检查儿童锁",{"$nulls":8},"01.取下不要的标签及覆盖物"]
["12.检查行李箱灯",{"$nulls":8},"02.检查内装部分的安装、污损情况"]
["13.行李箱内衬、垫板的检查",{"$nulls":8},"03.确认驾驶员手册等相关资料（欠品、误品等）"]
["14.检查备胎的气压和安装状况",{"$nulls":8},"04.安装轮毂盖"]
["15.检查千斤顶、工具、三角牌和牵引挂钩等",{"$nulls":8},"05.洗车、驾驶室内清扫"]
["16.引擎盖、车门的安装间隙、段差检查",{"$nulls":8},"06.检查漆面的不良、损坏情况"]
["17.检查驾驶席脚垫(如有)是否正确安装固定",{"$nulls":8},"07.检查外装部分的安装、损坏情况"]
[]
["C. 检查发动机仓"]
["01.检查油液类的量及其质量",{"$nulls":8},"外观备注"]
["  ·   发动机油"]
["    ·   转向助力油"]
["  ·  自动传动桥油"]
["  · 制动液、离合器液"]
["  ·  雨刷清洗液、防冻液"]
["  ·  电瓶液"]
["02.检查油类的渗漏情况"]
["03.检查电瓶桩头的安装情况"]
["04.测量电瓶的电压(                V、标准值12.2)"]
["05.检查电瓶充电情况"]
[]
["工 单 号：",{"$nulls":6},"备注"]
[]
["行驶公里："]
[{"$nulls":5},"KM"]
[]
[]
["检查员:",{"$nulls":6},"质检员:",{"$nulls":5},"服务部长确认:"]
[]
["VIN:",{"$nulls":6},"检查日期:",null,null,null,"经销商名称:",null,"驻马店威龙丰田汽车销售服务有限公司"]

{"sheet":"（2）新皇冠用PDS正版检查表","index":2,"n_rows":61,"n_cols":18,"rows_kept":61,"cut":false,"hidden":false,"merged":[[60,0,60,3],[0,0,1,17],[52,0,53,1],[54,0,55,1],[56,0,57,1]],"flags":["formulas_cached_only"]}
["皇冠新车检查表(PDS)"]
[]
[]
[{"$nulls":8},"调整",{"$nulls":8},"调整"]
["A. 作业准备",{"$nulls":6},"OK","修理","D. 下部检查",{"$nulls":6},"OK","修理"]
["01.轮胎气压计、扭力扳手、21寸套筒、万用表、工具",{"$nulls":8},"01.确认轮胎螺母的扭矩"]
["02.座套、翼子板布、把套、脚垫、布、垫板",{"$nulls":8},"02.调整轮胎的气压"]
["03.安装随车附件",{"$nulls":8},"03.检查轮胎的损坏情况"]
[{"$nulls":9},"04.安装随车附件"]
["B. 目视检查",{"$nulls":8},"05.拆除前弹簧隔垫、制动器防锈罩"]
["01.检查警告灯、蜂鸣器(钥匙、大灯)",{"$nulls":8},"06.检查油液类的渗漏情况"]
["02.检查发动机的起动性、稳定性、异音及振动",{"$nulls":8},"07.检查安装紧固情况"]
["03.电器件的工作状况",{"$nulls":8},"08.检查损伤、生锈情况"]
["    ·  大灯、小灯、雾灯、控制台灯光"]
["    ·  尾灯、牌照灯、后雾灯"]
["    ·  刹车灯、倒车灯、光束调整系统",{"$nulls":8},"E. 路  试"]
["  · 转向灯、双闪",{"$nulls":8},"01.检查踏板的游隙、高度和踩后余量"]
["  · 雨刷器、雨刷喷嘴、喇叭",{"$nulls":8},"02.检查发动机的起动性、平稳性、异响和振动(暖机)"]
["  · 除雾器、点烟器",{"$nulls":8},"03.行驶性能(加速、匀速、减速、灵敏性等)"]
["  · 音响(调频)、时钟(设为正确时间)",{"$nulls":8},"04.检查仪表、指示灯的工作情况"]
["  ·  遮阳板、化妆灯、地图灯",{"$nulls":8},"05.检查离合器、传动桥"]
["  ·  室内灯",{"$nulls":8},"06.检查制动性能、异响、驻车制动"]
["    ·  天窗动作",{"$nulls":8},"07.检查转向情况"]
["    ·  座椅加热情况",{"$nulls":8},"08.检查异响、噪音、振动、平稳性"]
["04.检查车内后视镜、门后视镜(调整为正常状态)",{"$nulls":8},"09.检查暖气、空调"]
["05.检查角度及高度可调方向盘动作",{"$nulls":8},"10.自动传动桥的检查"]
["06.检查储物箱及杯架、烟灰缸",{"$nulls":8},"11.检查卫星导航系统"]
["07.检查座椅、安全带的运作、污损情况",{"$nulls":8},"12.检查（雷达）巡航控制系统工作情况"]
["08.检查发动机盖、后备箱、加油孔盖的开启情况",{"$nulls":8},"13.检查智能泊车辅助系统工作状况"]
["09.检查车门玻璃的运作情况"]
["10.检查车门、门锁、遥控门锁、智能系统的工作情况",{"$nulls":8},"F. 最终检查、清洁"]
["11.检查儿童锁",{"$nulls":8},"01.取下不要的标签及覆盖物"]
["12.检查行李箱灯",{"$nulls":8},"02.检查内装部分的安装、污损情况"]
["13.行李箱内衬、垫板的检查",{"$nulls":8},"03.确认驾驶员手册等相关资料（欠品、误品等）"]
["14.检查备胎的气压和安装状况",{"$nulls":8},"04.安装轮毂盖"]
["15.检查千斤顶、工具、三角牌和牵引挂钩等",{"$nulls":8},"05.洗车、驾驶室内清扫"]
["16.引擎盖、车门的安装间隙、段差检查",{"$nulls":8},"06.检查漆面的不良、损坏情况"]
["17.检查驾驶席脚垫(如有)是否正确安装固定",{"$nulls":8},"07.检查外装部分的安装、损坏情况"]
[]
["C. 检查发动机仓"]
["01.检查油液类的量及其质量",{"$nulls":8},"外观备注"]
["  ·   发动机油"]
["    ·   转向助力油"]
["  ·  自动传动桥油"]
["  · 制动液、离合器液"]
["  ·  雨刷清洗液、防冻液"]
["  ·  电瓶液"]
["02.检查油类的渗漏情况"]
["03.检查电瓶桩头的安装情况"]
["04.测量电瓶的电压(                V、标准值12.2)"]
["05.检查电瓶充电情况"]
[]
["工 单 号：",{"$nulls":6},"备注"]
[]
["行驶公里："]
[{"$nulls":5},"KM"]
["VIN："]
[]
["检查员:",{"$nulls":6},"质检员:",{"$nulls":5},"服务部长确认:"]
[]
["皇冠检查证书发行日:",{"$nulls":6},"检查日期:",null,null,null,"经销商名称:",null,"驻马店威龙丰田汽车销售服务有限公司"]